**GPS database(radar detector) upgrade instructions**

1、Decompress the compressed file, Find to “LK181\_\*\*\*.exe” file;



2、gps database updating(The upgrade process does not allow midway power failure)：

①、copy “LK181\_\*\*\*.exe”file to computer,(computer needs to be 32 bits XP system, other system will probably not be available because of lacking configuration files).

Note: The solution cannot be upgraded


Solution 1: When the conditions permit, when the win7/win10 system is upgraded, the USB3.0 interface is used to upgrade the device. This can solve some problems that cannot be properly upgraded.

Solution 2: When the conditions permit, when the win7/win10 system is upgraded(Use a laptop to upgrade your device to your car) Supplying power to the device (first connected to DC power supply and then USB) can solve most problems that cannot be upgraded properly.

②、Connect device to computer by USB cable.（mini USB port）




③、 Check the computer "device manager（设备管理器）" → "human body input device" → "HID-compliant device（人体学输入设备）" (there is a successful connection to the computer, you can upgrade)




④、After computer recognizes USB serialport, double click“LK181\_\*\*\*.exe”file.




Step 1：click“Next（N）”button





Step 2: click“Start（S）”button




Step 3：waiting for finishing updating










Step 4：see“Updata success”，it means updating finishes.

Note: Do not disconnect the USB connection, wait 5 seconds,next step.



Step 5： Click “Quit（C）”button to exit, firmware updating finishes.