# Caractéristiques

Interface Bluetooth principale prise en charge :

HCI (Host Controller Interface) v3.0 + High Speed (HS)

Profils Bluetooth pris en charge :

- A2DP (Advanced Audio Distribution Profile) (Source/Récepteur)
- AVRCP (A/V Remote Control Profile) (Contrôleur/Cible)
- FTP (File Transfer Profil) (Client/Serveur)
- GAVDP (Generic A/V Distribution Profile) (Source)
- GOEP (Generic Object Exchange Profile) (Client/Serveur)
- HFP (Hands-Free Profile) (Passerelle audio)
- HSP (Headset Profile) (Passerelle audio)
- SYNC (Synchronization Profile) (Client)
- BIP (Basic Imaging Profile) (Push Responder)
- BPP (Basic Printing Profile) (Émetteur)
- Client PBAP (Phone Book Access Profile) et SYNCH (Synchronization Profile)
- VDP (Video Distribution Profile) (Source/Récepteur)

Systèmes d'exploitation :

- Windows Vista (32 bits et 64 bits) SP2
- Windows 7 (32 bits et 64 bits)

Langues prises en charge :

- Arabe
- Chinois simplifié
- Chinois traditionnel
- Tchèque
- Danois
- Néerlandais
- Anglais
- Finnois
- Français
- Allemand
- Grec
- Hébreu
- Hongrois
- Italien
- Japonais
- Coréen
- Norvégien
- Polonais
- Portugais (Brésil)
- Portugais (Europe)
- Russe
- Espagnol
- Suédois
- Thaïlandais
- Turc

Liste des acronymes :

- A2DP – Advanced Audio Distribution Profile
- AFH – Adaptive Frequency-Hopping (Étalement de spectre)
- AMP – Alternate MAC/PHY
- AVRCP – Audio/Video Remote Control Profile
- BIP – Basic Imaging Profile
- BPP – Basic Printing Profile
- DRM – Digital Rights Management
- EDR – Enhanced Data Rate
- FTP – File Transfer Protocol
- HFP – Hands-Free Profile
- HS – High Speed
- HSP – Headset Profile
- MAC/PHY – Media Access Control/Physical Layer
- PBAP – Phone Book Access Profile
- OBEX – Object Exchange
- PBAP – Phone Book Access Profile
- SCMS-T – Serial Copy Management System
- SYNCH – Synchronization Profile
- SRM – Single Response Mode
- VDP – Video Distribution Profile
- VoIP – Voice over IP