
**Car DVR upgrade instructions**

1、Decompress the compressed file, Find to “SD\_CarDV.bin” file;




2、Car DVR updating steps(The upgrade process does not allow midway power failure):


①、copy“SD\_CarDV.bin”file into SD card(Class6 above).

②、Insert SD card into device, then connect power for device. It will take about 1 min and 30S to 2 min and 30S or so to finish updating, specific steps are below:


Step 1：Read File，waiting for progress bar to finish.



Step 2：Write firmware，waiting for progress bar to finish.



Step 3：Write Done，waiting for progress bar to finish.



Step 4：after finish steps above, the screen of device will become black, please wait for 5 seconds, then cut off power, pull out TF card, firmware updating will be done.

Step 5：Format SD card which includes “SD\_CarDV.bin”file on computer，then the SD card can be used normally in device.